|  |  |
| --- | --- |
| Logo_col | Bundesamt für Zivilluftfahrt BAZLOffice fédérale de l’aviation civile OFACUfficio federale dell’aviazione civile UFACFederal Office of Civil Aviation FOCA |

CAT.SEC./IDE.H Compliance

|  |
| --- |
| BAZL Form: |
| CAT.SEC./IDE.H Compliance |
| Revision: | Revision date: | Prepared by: | Released by: | Distribution: |
| 8 | 04.2020 | fro | hav | STLB |

|  |
| --- |
| Reference: |
| Excerpts of Basic Regulation EC 2018/1139 amended by |
| ID: | Publication: | Publication date: | Remarks: |
|  |  |  |  |
| Commission Regulation (EU) No 965/2012 amended by |
| ID: | Publication: | Publication date: | Remarks: |
| 15 | 2019/1387 | 05/09/2019 |  |

**Contents**

[CAT.SEC./IDE.H Compliance 0](#_Toc38459044)

[General 4](#_Toc38459045)

[Reference 4](#_Toc38459046)

[Introduction 4](#_Toc38459047)

[Purpose 4](#_Toc38459048)

[Applicability 4](#_Toc38459049)

[Completion 4](#_Toc38459050)

[Applicant details 5](#_Toc38459051)

[Applicant 5](#_Toc38459052)

[Aircraft 5](#_Toc38459053)

[EASA OPS Requirement 6](#_Toc38459054)

[ORO.SEC.105 Flight crew compartment security 6](#_Toc38459055)

[CAT.IDE.H.100 Instruments and equipment - general 6](#_Toc38459056)

[CAT.IDE.H.105 Minimum equipment for flight 8](#_Toc38459057)

[CAT.IDE.H.115 Operating lights 8](#_Toc38459058)

[CAT.IDE.H.125 Operations under VFR by day flight and navigational instruments and associated equipment 9](#_Toc38459059)

[CAT.IDE.H.130 Operations under IFR or at night flight and navigational instruments and associated equipment 10](#_Toc38459060)

[CAT.IDE.H.135 Additional equipment for single pilot operation under IFR 12](#_Toc38459061)

[CAT.IDE.H.145 Radio altimeters 13](#_Toc38459062)

[CAT.IDE.H.160 Airborne weather detecting equipment 13](#_Toc38459063)

[CAT.IDE.H.165 Additional equipment for operations in icing conditions at night 14](#_Toc38459064)

[CAT.IDE.H.170 Flight crew interphone system 14](#_Toc38459065)

[CAT.IDE.H.175 Crew member interphone system 15](#_Toc38459066)

[CAT.IDE.H.180 Public address system 15](#_Toc38459067)

[CAT.IDE.H.185 Cockpit voice recorder 16](#_Toc38459068)

[CAT.IDE.H.190 Flight data recorder 18](#_Toc38459069)

[CAT.IDE.H.191 Lightweight flight recorder 19](#_Toc38459070)

[CAT.IDE.H.195 Data link recording 20](#_Toc38459071)

[CAT.IDE.H.200 Flight data and cockpit voice combination recorder 21](#_Toc38459072)

[CAT.IDE.H.205 Seats, seat safety belts, restraint systems and child restraint devices 22](#_Toc38459073)

[CAT.IDE.H.210 Fasten seat belt and no smoking signs 23](#_Toc38459074)

[CAT.IDE.H.220 First-aid kits 23](#_Toc38459075)

[CAT.IDE.H.240 Supplemental oxygen — non-pressurised helicopters 24](#_Toc38459076)

[CAT.IDE.H.250 Hand fire extinguishers 25](#_Toc38459077)

[CAT.IDE.H.260 Marking of break-in points 26](#_Toc38459078)

[CAT.IDE.H.270 Megaphones 27](#_Toc38459079)

[CAT.IDE.H.275 Emergency lighting and marking 27](#_Toc38459080)

[CAT.IDE.H.280 Emergency locator transmitter (ELT) 28](#_Toc38459081)

[CAT.IDE.H.290 Life-jackets 28](#_Toc38459082)

[CAT.IDE.H.295 Crew survival suits 29](#_Toc38459083)

[CAT.IDE.H.300 Life-rafts, survival ELTs and survival equipment on extended overwater flights 30](#_Toc38459084)

[CAT.IDE.H.305 Survival equipment 31](#_Toc38459085)

[CAT.IDE.H.315 Helicopters certified for operating on water — miscellaneous equipment 31](#_Toc38459086)

[CAT.IDE.H.320 All helicopters on flights over water — ditching 32](#_Toc38459087)

[CAT.IDE.H.325 Headset 33](#_Toc38459088)

[CAT.IDE.H.330 Radio communication equipment 33](#_Toc38459089)

[CAT.IDE.H.335 Audio selector panel 34](#_Toc38459090)

[CAT.IDE.H.340 Radio equipment for operations under VFR over routes navigated by reference to visual landmarks 34](#_Toc38459091)

[CAT.IDE.H.345 Communication and navigation equipment for operations under IFR or under VFR over routes not navigated by reference to visual landmarks 35](#_Toc38459092)

[CAT.IDE.H.350 Transponder 36](#_Toc38459093)

[CAT.IDE.H.355 Management of aeronautical databases 37](#_Toc38459094)

[Applicant’s Statement 38](#_Toc38459095)

# General

## Reference

This compliance List is derived from EASA Regulation (EC) 2018/1139 and 965/2012 respectively (current issue).

## Introduction

Aircraft may be imported into Switzerland, provided it can be shown that the aircraft conforms to EASA Air Operations Regulation Annex III and IV -ORO.SEC-/CAT.IDE.H

## Purpose

The intent of this compliance list is to ensure that an aircraft to be operated commercially (EC N1321/2014 Article 1(3)/ EC No EC No 1008/2008) has been examined by the operator and is considered in conformity with the above mentioned requirements. The text of the corresponding requirement (LH Column) has been shortened and should be used for reference only.

## Applicability

Import of new or used aircraft, export or dry lease-in of used aircraft, change of operator or new operation under AOC within Switzerland.

For all operators / holders of aircraft operated commercially (EC No 1321/2014 Article 1(3) / EC No 1008/2008.

## Completion

Note 1: Each relevant box to be completed with a cross (X). If the relevant ORO.SEC-/CAT.IDE.H paragraph is not applicable to aircraft registration, complete column N/A(Not Applicable) with a cross (X)

Note 2: Add STC number (i.e. STC 12345-LA)

Note 3: Add reference of service publication and revision number or revision date (i.e. SB 25-123 Rev. 2)

Note 4: If Note 2 and Note 3 not applicable add references of other compliance documents (i.e. Mod. 6789)

Submit form to: **Federal Office of Civil Aviation**

**Safety Division Aircraft**

**Section Airworthiness**

**CH-3003 Berne**

# Applicant details

## Applicant

|  |  |  |  |
| --- | --- | --- | --- |
| Operator |       | Aircraft Registration |       |

## Aircraft

|  |  |  |  |
| --- | --- | --- | --- |
| Manufacturer |       | Type Designation |       |
| Serial No. |       | Year of Manufacture |       |
| MTOM (kg) |       | MOPSC (\*) |       |
| TCDS |       | Engine |       |

(\*) MOPSC: Maximum Operated Passenger Seat Capacity

# EASA OPS Requirement

## ORO.SEC.105 Flight crew compartment security

|  |  |
| --- | --- |
| **Declaration of Compliance** | **Means of Compliance** |
|  | Requirement Satisfied | Requirement satisfied through type design as specified in Type Certificate Data Sheet (TCDS) | Requirement satisfied through Supplemental Type Certificate (STC) Process | Requirement satisfied through embodiment of manufacturer service publications (Service Bulletins, Service Changes, etc.) | Other  |
|  | (Note 1-4) | (Note 1) | (Note 2) | (Note 3) | (Note 4) |
|  | **Yes** | **N/A** |  |
| If installed, the flight crew compartment door on a helicopter operated for the purpose of carrying passengers shall be capable of being locked from within the flight crew compartment in order to prevent unauthorized access. |[ ] [ ] [ ]        |       |       |

## CAT.IDE.H.100 Instruments and equipment - general

|  |  |
| --- | --- |
| **Declaration of Compliance** | **Means of Compliance** |
| 1. Instruments and equipment required by this Subpart shall be approved in accordance with the applicable airworthiness requirements, except for the following items:
 | Requirement Satisfied | Requirement satisfied through type design as specified in Type Certificate Data Sheet (TCDS) | Requirement satisfied through Supplemental Type Certificate (STC) Process | Requirement satisfied through embodiment of manufacturer service publications (Service Bulletins, Service Changes, etc.) | Other  |
|  | (Note 1-4) | (Note 1) | (Note 2) | (Note 3) | (Note 4) |
|  | **Yes** | **N/A** |  |
| 1. Independent portable lights;
 |[ ] [ ] [ ]        |       |       |
| 1. An accurate time piece;
 |[ ] [ ] [ ]        |       |       |
| 1. Chart holder;
 |[ ] [ ] [ ]        |       |       |
| 1. First-aid kit;
 |[ ] [ ] [ ]        |       |       |
| 1. Megaphones;
 |[ ] [ ] [ ]        |       |       |
| 1. Survival and signaling equipment;
 |[ ] [ ] [ ]        |       |       |
| 1. Sea anchors and equipment for mooring;
 |[ ] [ ] [ ]        |       |       |
| 1. Child restraint devices.
 |[ ] [ ] [ ]        |       |       |
| 1. Instruments and equipment not required under this Annex (Part-CAT) as well as any other equipment which is not required under this Regulation, but carried on a flight, shall comply with the following requirements:
 |  |
| 1. the information provided by those instruments, equipment or accessories shall not be used by the flight crew members to comply with Annex II to Regulation (EU) No 2018/1139 or points CAT.IDE.H.330, CAT.IDE.H.335, CAT.IDE.H.340 and CAT.IDE.H.345 of this Annex;
 |[ ] [ ] [ ]        |       |       |
| 1. the instruments and equipment shall not affect the airworthiness of the helicopter, even in the case of failures or malfunction.
 |[ ] [ ] [ ]        |       |       |
| 1. If equipment is to be used by one flight crew member at his/her station during flight, it shall be readily operable from that station. When a single item of equipment is required to be operated by more than one flight crew member it shall be installed so that the equipment is readily operable from any station at which the equipment is required to be operated.
 |[ ] [ ] [ ]        |       |       |
| 1. Those instruments that are used by any flight crew member shall be so arranged as to permit the flight crew member to see the indications readily from his/her station, with the minimum practicable deviation from the position and line of vision that he/she normally assumes when looking forward along the flight path.
 |[ ] [ ] [ ]        |       |       |
| 1. All required emergency equipment shall be easily accessible for immediate use.
 |[ ] [ ] [ ]        |       |       |

## CAT.IDE.H.105 Minimum equipment for flight

|  |  |
| --- | --- |
| **Declaration of Compliance** | **Means of Compliance** |
| A flight shall not be commenced when any of the helicopter's instruments, items of equipment or functions required for the intended flight are inoperative or missing, unless: | Requirement Satisfied | Requirement satisfied through type design as specified in Type Certificate Data Sheet (TCDS) | Requirement satisfied through Supplemental Type Certificate (STC) Process | Requirement satisfied through embodiment of manufacturer service publications (Service Bulletins, Service Changes, etc.) | Other  |
|  | (Note 1-4) | (Note 1) | (Note 2) | (Note 3) | (Note 4) |
|  | **Yes** | **N/A** |  |
| 1. the helicopter is operated in accordance with the operator's MEL; or
 |[ ] [ ] [ ]        |       |       |
| 1. the operator is approved by the competent authority to operate the helicopter within the constraints of the MMEL in accordance with point ORO.MLR.105(j) of Annex III.
 |[ ] [ ] [ ]        |       |       |

## CAT.IDE.H.115 Operating lights

|  |  |
| --- | --- |
| **Declaration of Compliance** | **Means of Compliance** |
|  | Requirement Satisfied | Requirement satisfied through type design as specified in Type Certificate Data Sheet (TCDS) | Requirement satisfied through Supplemental Type Certificate (STC) Process | Requirement satisfied through embodiment of manufacturer service publications (Service Bulletins, Service Changes, etc.) | Other  |
|  | (Note 1-4) | (Note 1) | (Note 2) | (Note 3) | (Note 4) |
|  | **Yes** | **N/A** |  |
| 1. Helicopters operated under VFR by day shall be equipped with an anti-collision light system.
 |[ ] [ ] [ ]        |       |       |
| 1. Helicopters operated at night or under IFR shall, in addition to (a), be equipped with:
 |  |
| 1. lighting supplied from the helicopter's electrical system to provide adequate illumination for all instruments and equipment essential to the safe operation of the helicopter;
 |[ ] [ ] [ ]        |       |       |
| 1. lighting supplied from the helicopter's electrical system to provide illumination in all passenger compartments;
 |[ ] [ ] [ ]        |       |       |
| 1. an independent portable light for each required crew member readily accessible to crew members when seated at their designated stations;
 |[ ] [ ] [ ]        |       |       |
| 1. navigation/position lights;
 |[ ] [ ] [ ]        |       |       |
| 1. two landing lights of which at least one is adjustable in flight so as to illuminate the ground in front of and below the helicopter and the ground on either side of the helicopter; and
 |[ ] [ ] [ ]        |       |       |
| 1. lights to conform with the International Regulations for Preventing Collisions at Sea if the helicopter is amphibious.
 |[ ] [ ] [ ]        |       |       |

## CAT.IDE.H.125 Operations under VFR by day flight and navigational instruments and associated equipment

|  |  |
| --- | --- |
| **Declaration of Compliance** | **Means of Compliance** |
| 1. Helicopters operated under VFR by day shall be equipped with the following equipment, available at the pilot's station:
 | Requirement Satisfied | Requirement satisfied through type design as specified in Type Certificate Data Sheet (TCDS) | Requirement satisfied through Supplemental Type Certificate (STC) Process | Requirement satisfied through embodiment of manufacturer service publications (Service Bulletins, Service Changes, etc.) | Other  |
|  | (Note 1-4) | (Note 1) | (Note 2) | (Note 3) | (Note 4) |
|  | **Yes** | **N/A** |  |
| 1. A means of measuring and displaying:
 |  |
| 1. Magnetic heading;
 |[ ] [ ] [ ]        |       |       |
| 1. Time in hours, minutes, and seconds;
 |[ ] [ ] [ ]        |       |       |
| 1. Barometric altitude;
 |[ ] [ ] [ ]        |       |       |
| 1. Indicated airspeed;
 |[ ] [ ] [ ]        |       |       |
| 1. Vertical speed;
 |[ ] [ ] [ ]        |       |       |
| 1. Slip; and
 |[ ] [ ] [ ]        |       |       |
| 1. Outside air temperature.
 |[ ] [ ] [ ]        |       |       |
| 1. A means of indicating when the supply of power to the required flight instruments is not adequate.
 |[ ] [ ] [ ]        |       |       |
| 1. Whenever two pilots are required for the operation, an additional separate means of displaying the following shall be available for the second pilot:
 |  |
| 1. Barometric altitude;
 |[ ] [ ] [ ]        |       |       |
| 1. Indicated airspeed;
 |[ ] [ ] [ ]        |       |       |
| 1. Vertical speed; and
 |[ ] [ ] [ ]        |       |       |
| 1. Slip.
 |[ ] [ ] [ ]        |       |       |
| 1. Helicopters with an MCTOM of more than 3’175 kg or any helicopter operating over water when out of sight of land or when the visibility is less than 1’500 m, shall be equipped with a means of measuring and displaying:
 |  |
| 1. Attitude; and
 |[ ] [ ] [ ]        |       |       |
| 1. Heading
 |[ ] [ ] [ ]        |       |       |
| 1. A means for preventing malfunction of the airspeed indicating systems due to condensation or icing shall be available for helicopters with an MCTOM of more than 3’175 kg or an MOPSC of more than nine.
 |[ ] [ ] [ ]        |       |       |

## CAT.IDE.H.130 Operations under IFR or at night flight and navigational instruments and associated equipment

|  |  |
| --- | --- |
| **Declaration of Compliance** | **Means of Compliance** |
| Helicopters operated under VFR at night or under IFR shall be equipped with the following equipment, available at the pilot's station: | Requirement Satisfied | Requirement satisfied through type design as specified in Type Certificate Data Sheet (TCDS) | Requirement satisfied through Supplemental Type Certificate (STC) Process | Requirement satisfied through embodiment of manufacturer service publications (Service Bulletins, Service Changes, etc.) | Other  |
|  | (Note 1-4) | (Note 1) | (Note 2) | (Note 3) | (Note 4) |
|  | **Yes** | **N/A** |  |
| 1. A means of measuring and displaying:
 |  |
| 1. Magnetic heading;
 |[ ] [ ] [ ]        |       |       |
| 1. Time in hours, minutes and seconds;
 |[ ] [ ] [ ]        |       |       |
| 1. Indicated airspeed;
 |[ ] [ ] [ ]        |       |       |
| 1. Vertical speed;
 |[ ] [ ] [ ]        |       |       |
| 1. Slip;
 |[ ] [ ] [ ]        |       |       |
| 1. Attitude;
 |[ ] [ ] [ ]        |       |       |
| 1. Stabilized heading; and
 |[ ] [ ] [ ]        |       |       |
| 1. Outside air temperature.
 |[ ] [ ] [ ]        |       |       |
| 1. Two means of measuring and displaying barometric altitude. For single-pilot operations under VFR at night one pressure altimeter may be substituted by a radio altimeter.
 |[ ] [ ] [ ]        |       |       |
| 1. A means of indicating when the supply of power to the required flight instruments is not adequate.
 |[ ] [ ] [ ]        |       |       |
| 1. A means of preventing malfunction of the airspeed indicating systems required in (a)(3) and (h)(2) due to either condensation or icing.
 |[ ] [ ] [ ]        |       |       |
| 1. A means of annunciating to the flight crew the failure of the means required in (d) for helicopters:
 |  |
| 1. issued with an individual CofA on or after 1 August 1999; or
 |[ ] [ ] [ ]        |       |       |
| 1. issued with an individual CofA before 1 August 1999 with an MCTOM of more than 3’175 kg, and with an MOPSC of more than nine.
 |[ ] [ ] [ ]        |       |       |
| 1. A standby means of measuring and displaying attitude that:
 |  |
| 1. is powered continuously during normal operation and, in the event of a total failure of the normal electrical generating system, is powered from a source independent of the normal electrical generating system;
 |[ ] [ ] [ ]        |       |       |
| 1. operates independently of any other means of measuring and displaying attitude;
 |[ ] [ ] [ ]        |       |       |
| 1. is capable of being used from either pilot's station;
 |[ ] [ ] [ ]        |       |       |
| 1. is operative automatically after total failure of the normal electrical generating system;
 |[ ] [ ] [ ]        |       |       |
| 1. provides reliable operation for a minimum of 30 minutes or the time required to fly to a suitable alternate landing site when operating over hostile terrain or offshore, whichever is greater, after total failure of the normal electrical generating system, taking into account other loads on the emergency power supply and operational procedures;
 |[ ] [ ] [ ]        |       |       |
| 1. is appropriately illuminated during all phases of operation; and
 |[ ] [ ] [ ]        |       |       |
| 1. is associated with a means to alert the flight crew when operating under its dedicated power supply, including when operated by emergency power.
 |[ ] [ ] [ ]        |       |       |
| 1. An alternate source of static pressure for the means of measuring altitude, airspeed and vertical speed.
 |[ ] [ ] [ ]        |       |       |
| 1. Whenever two pilots are required for the operation, a separate means for displaying for the second pilot:
 |  |
| 1. Barometric altitude;
 |[ ] [ ] [ ]        |       |       |
| 1. Indicated airspeed;
 |[ ] [ ] [ ]        |       |       |
| 1. Vertical speed;
 |[ ] [ ] [ ]        |       |       |
| 1. Slip;
 |[ ] [ ] [ ]        |       |       |
| 1. Attitude; and
 |[ ] [ ] [ ]        |       |       |
| 1. Stabilized heading.
 |[ ] [ ] [ ]        |       |       |
| 1. For IFR operations, a chart holder in an easily readable position that can be illuminated for night operations.
 |[ ] [ ] [ ]        |       |       |

## CAT.IDE.H.135 Additional equipment for single pilot operation under IFR

|  |  |
| --- | --- |
| **Declaration of Compliance** | **Means of Compliance** |
|  | Requirement Satisfied | Requirement satisfied through type design as specified in Type Certificate Data Sheet (TCDS) | Requirement satisfied through Supplemental Type Certificate (STC) Process | Requirement satisfied through embodiment of manufacturer service publications (Service Bulletins, Service Changes, etc.) | Other  |
|  | (Note 1-4) | (Note 1) | (Note 2) | (Note 3) | (Note 4) |
|  | **Yes** | **N/A** |  |  |  |  |
| Helicopters operated under IFR with a single-pilot shall be equipped with an autopilot with at least altitude hold and heading mode. |[ ] [ ] [ ]        |       |       |

## CAT.IDE.H.145 Radio altimeters

|  |  |
| --- | --- |
| **Declaration of Compliance** | **Means of Compliance** |
| Helicopters on flights over water shall be equipped with a radio altimeter capable of emitting an audio warning below a pre-set height and a visual warning at a height selectable by the pilot, when operating: | Requirement Satisfied | Requirement satisfied through type design as specified in Type Certificate Data Sheet (TCDS) | Requirement satisfied through Supplemental Type Certificate (STC) Process | Requirement satisfied through embodiment of manufacturer service publications (Service Bulletins, Service Changes, etc.) | Other  |
|  | (Note 1-4) | (Note 1) | (Note 2) | (Note 3) | (Note 4) |
|  | **Yes** | **N/A** |  |  |  |  |
| 1. out of sight of the land;
 |[ ] [ ] [ ]        |       |       |
| 1. in a visibility of less than 1’500 m;
 |[ ] [ ] [ ]        |       |       |
| 1. at night; or
 |[ ] [ ] [ ]        |       |       |
| 1. at a distance from land corresponding to more than three minutes at normal cruising speed.
 |[ ] [ ] [ ]        |       |       |

## CAT.IDE.H.160 Airborne weather detecting equipment

|  |  |
| --- | --- |
| **Declaration of Compliance** | **Means of Compliance** |
|  | Requirement Satisfied | Requirement satisfied through type design as specified in Type Certificate Data Sheet (TCDS) | Requirement satisfied through Supplemental Type Certificate (STC) Process | Requirement satisfied through embodiment of manufacturer service publications (Service Bulletins, Service Changes, etc.) | Other  |
|  | (Note 1-4) | (Note 1) | (Note 2) | (Note 3) | (Note 4) |
|  | **Yes** | **N/A** |  |  |  |  |
| Helicopters with an MOPSC of more than nine and operated under IFR or at night shall be equipped with airborne weather detecting equipment when current weather reports indicate that thunderstorms or other potentially hazardous weather conditions, regarded as detectable with airborne weather detecting equipment, may be expected to exist along the route to be flown. |[ ] [ ] [ ]        |       |       |

## CAT.IDE.H.165 Additional equipment for operations in icing conditions at night

|  |  |
| --- | --- |
| **Declaration of Compliance** | **Means of Compliance** |
|  | Requirement Satisfied | Requirement satisfied through type design as specified in Type Certificate Data Sheet (TCDS) | Requirement satisfied through Supplemental Type Certificate (STC) Process | Requirement satisfied through embodiment of manufacturer service publications (Service Bulletins, Service Changes, etc.) | Other  |
|  | (Note 1-4) | (Note 1) | (Note 2) | (Note 3) | (Note 4) |
|  | **Yes** | **N/A** |  |  |  |  |
| 1. Helicopters operated in expected or actual icing conditions at night shall be equipped with a means to illuminate or detect the formation of ice.
 |[ ] [ ] [ ]        |       |       |
| 1. The means to illuminate the formation of ice shall not cause glare or reflection that would handicap crew members in the performance of their duties.
 |[ ] [ ] [ ]        |       |       |

## CAT.IDE.H.170 Flight crew interphone system

|  |  |
| --- | --- |
| **Declaration of Compliance** | **Means of Compliance** |
|  | Requirement Satisfied | Requirement satisfied through type design as specified in Type Certificate Data Sheet (TCDS) | Requirement satisfied through Supplemental Type Certificate (STC) Process | Requirement satisfied through embodiment of manufacturer service publications (Service Bulletins, Service Changes, etc.) | Other  |
|  | (Note 1-4) | (Note 1) | (Note 2) | (Note 3) | (Note 4) |
|  | **Yes** | **N/A** |  |  |  |  |
| Helicopters operated by more than one flight crew member shall be equipped with a flight crew interphone system, including headsets and microphones for use by all flight crew members. |[ ] [ ] [ ]        |       |       |

## CAT.IDE.H.175 Crew member interphone system

|  |  |
| --- | --- |
| **Declaration of Compliance** | **Means of Compliance** |
|  | Requirement Satisfied | Requirement satisfied through type design as specified in Type Certificate Data Sheet (TCDS) | Requirement satisfied through Supplemental Type Certificate (STC) Process | Requirement satisfied through embodiment of manufacturer service publications (Service Bulletins, Service Changes, etc.) | Other  |
|  | (Note 1-4) | (Note 1) | (Note 2) | (Note 3) | (Note 4) |
|  | **Yes** | **N/A** |  |  |  |  |
| Helicopters shall be equipped with a crew member interphone system when carrying a crew member other than a flight crew member. |[ ] [ ] [ ]        |       |       |

## CAT.IDE.H.180 Public address system

|  |  |
| --- | --- |
| **Declaration of Compliance** | **Means of Compliance** |
|  | Requirement Satisfied | Requirement satisfied through type design as specified in Type Certificate Data Sheet (TCDS) | Requirement satisfied through Supplemental Type Certificate (STC) Process | Requirement satisfied through embodiment of manufacturer service publications (Service Bulletins, Service Changes, etc.) | Other  |
|  | (Note 1-4) | (Note 1) | (Note 2) | (Note 3) | (Note 4) |
|  | **Yes** | **N/A** |  |  |  |  |
| 1. Helicopters with an MOPSC of more than nine shall be equipped with a public address system, with the exception of (b).
 |[ ] [ ] [ ]        |       |       |
| 1. Notwithstanding (a) helicopters with an MOPSC of more than nine and less than 20 are exempted from having a public address system, if:
 |  |
| 1. the helicopter is designed without a bulkhead between pilot and passengers; and
 |[ ] [ ] [ ]        |       |       |
| 1. the operator is able to demonstrate that when in flight, the pilot's voice is audible and intelligible at all passengers' seats.
 |[ ] [ ] [ ]        |       |       |

## CAT.IDE.H.185 Cockpit voice recorder

|  |  |
| --- | --- |
| **Declaration of Compliance** | **Means of Compliance** |
| 1. The following helicopter types shall be equipped with a cockpit voice recorder (CVR):
 | Requirement Satisfied | Requirement satisfied through type design as specified in Type Certificate Data Sheet (TCDS) | Requirement satisfied through Supplemental Type Certificate (STC) Process | Requirement satisfied through embodiment of manufacturer service publications (Service Bulletins, Service Changes, etc.) | Other  |
|  | (Note 1-4) | (Note 1) | (Note 2) | (Note 3) | (Note 4) |
|  | **Yes** | **N/A** |  |  |  |  |
| 1. all helicopters with an MCTOM of more than 7’000 Kg; and
 |[ ] [ ] [ ]        |       |       |
| 1. helicopters with an MCTOM of more than 3’175 Kg and first issued with an individual CofA on or after 1 January 1987.
 |[ ] [ ] [ ]        |       |       |
| 1. The CVR shall be capable of retaining the data recorded during at least:
 |  |
| 1. the preceding two hours for helicopters referred to in (a)(1) and (a)(2), when first issued with an individual CofA on or after 1 January 2016;
 |[ ] [ ] [ ]        |       |       |
| 1. the preceding one hour for helicopters referred to in (a)(1), when first issued with an individual CofA on or after 1 August 1999 and before 1 January 2016;
 |[ ] [ ] [ ]        |       |       |
| 1. the preceding 30 minutes for helicopters referred to in (a)(1), when first issued with an individual CofA before 1 August 1999; or
 |[ ] [ ] [ ]        |       |       |
| 1. the preceding 30 minutes for helicopters referred to in (a)(2), when first issued with an individual CofA before 1 January 2016.
 |[ ] [ ] [ ]        |       |       |
| 1. By 1 January 2019 at the latest, the CVR shall record on means other than magnetic tape or magnetic wire.
 |[ ] [ ] [ ]        |       |       |
| 1. The CVR shall record with reference to a timescale:
 |  |
| 1. voice communications transmitted from or received in the flight crew compartment by radio;
 |[ ] [ ] [ ]        |       |       |
| 1. flight crew members' voice communications using the interphone system and the public address system, if installed;
 |[ ] [ ] [ ]        |       |       |
| 1. the aural environment of the flight crew compartment, including without interruption:
 |  |
| 1. for helicopters first issued with an individual CofA on or after 1 August 1999, the audio signals received from each crew microphone;
 |[ ] [ ] [ ]        |       |       |
| 1. for helicopters first issued with an individual CofA before 1 August 1999, the audio signals received from each crew microphone, where practicable;
 |[ ] [ ] [ ]        |       |       |
| 1. voice or audio signals identifying navigation or approach aids introduced into a headset or speaker.
 |[ ] [ ] [ ]        |       |       |
| 1. The CVR shall start to record prior to the helicopter moving under its own power and shall continue to record until the termination of the flight when the helicopter is no longer capable of moving under its own power.
 |[ ] [ ] [ ]        |       |       |
| 1. In addition to (e), for helicopters referred to in (a)(2) issued with an individual CofA on or after 1 August 1999:
 |  |
| 1. the CVR shall start automatically to record prior to the helicopter moving under its own power and continue to record until the termination of the flight when the helicopter is no longer capable of moving under its own power; and
 |[ ] [ ] [ ]        |       |       |
| 1. depending on the availability of electrical power, the CVR shall start to record as early as possible during the cockpit checks prior to engine start at the beginning of the flight until the cockpit checks immediately following engine shutdown at the end of the flight.
 |[ ] [ ] [ ]        |       |       |
| 1. If the CVR is not deployable, it shall have a device to assist in locating it under water. By 1 January 2020 at the latest, this device shall have a minimum underwater transmission time of 90 days. If the CVR is deployable, it shall have an automatic emergency locator transmitter.
 |[ ] [ ] [ ]        |       |       |

## CAT.IDE.H.190 Flight data recorder

|  |  |
| --- | --- |
| **Declaration of Compliance** | **Means of Compliance** |
| 1. The following helicopters shall be equipped with an FDR that uses a digital method of recording and storing data and for which a method of readily retrieving that data from the storage medium is available:
 | Requirement Satisfied | Requirement satisfied through type design as specified in Type Certificate Data Sheet (TCDS) | Requirement satisfied through Supplemental Type Certificate (STC) Process | Requirement satisfied through embodiment of manufacturer service publications (Service Bulletins, Service Changes, etc.) | Other  |
|  | (Note 1-4) | (Note 1) | (Note 2) | (Note 3) | (Note 4) |
|  | **Yes** | **N/A** |  |  |  |  |
| 1. helicopters with an MCTOM of more than 3’175 kg and first issued with an individual CofA on or after 1 August 1999;
 |[ ] [ ] [ ]        |       |       |
| 1. helicopters with an MCTOM of more than 7’000 kg, or an MOPSC of more than nine, and first issued with an individual CofA on or after 1 January 1989 but before 1 August 1999.
 |[ ] [ ] [ ]        |       |       |
| 1. The FDR shall record the parameters required to determine accurately the:
 |  |
| 1. flight path, speed, attitude, engine power, operation and configuration and be capable of retaining the data recorded during at least the preceding 10 hours, for helicopters referred to in (a)(1) and first issued with an individual CofA on or after 1 January 2016;
 |[ ] [ ] [ ]        |       |       |
| 1. flight path, speed, attitude, engine power and operation and be capable of retaining the data recorded during at least the preceding eight hours, for helicopters referred to in (a)(1) and first issued with an individual CofA before 1 January 2016;
 |[ ] [ ] [ ]        |       |       |
| 1. flight path, speed, attitude, engine power and operation and be capable of retaining the data recorded during at least the preceding five hours, for helicopters referred to in (a)(2).
 |[ ] [ ] [ ]        |       |       |
| 1. Data shall be obtained from helicopter sources that enable accurate correlation with information displayed to the flight crew.
 |[ ] [ ] [ ]        |       |       |
| 1. The FDR shall automatically start to record the data prior to the helicopter being capable of moving under its own power and shall stop automatically after the helicopter is incapable of moving under its own power.
 |[ ] [ ] [ ]        |       |       |
| 1. If the FDR is not deployable, it shall have a device to assist in locating it under water. By 1 January 2020 at the latest, this device shall have a minimum underwater transmission time of 90 days. If the FDR is deployable, it shall have an automatic emergency locator transmitter.
 |[ ] [ ] [ ]        |       |       |

## CAT.IDE.H.191 Lightweight flight recorder

|  |  |
| --- | --- |
| **Declaration of Compliance** | **Means of Compliance** |
| 1. Turbine-engined helicopters with an MCTOM of 2 250 kg or more shall be equipped with a flight recorder if all of the following conditions are met:
 | Requirement Satisfied | Requirement satisfied through type design as specified in Type Certificate Data Sheet (TCDS) | Requirement satisfied through Supplemental Type Certificate (STC) Process | Requirement satisfied through embodiment of manufacturer service publications (Service Bulletins, Service Changes, etc.) | Other  |
|  | (Note 1-4) | (Note 1) | (Note 2) | (Note 3) | (Note 4) |
|  | **Yes** | **N/A** |  |  |  |  |
| 1. they are not within the scope of point CAT.IDE.H.190(a);
 |  |
| 1. they are first issued with an individual CofA on or after 5 September 2022.
 |[ ] [ ] [ ]        |       |       |
| 1. The flight recorder shall record, by means of flight data or images, information that is sufficient to determine the flight path and aircraft speed.
 |[ ] [ ] [x]        |       |       |
| 1. The flight recorder shall be capable of retaining the flight data and the images recorded during at least the preceding 5 hours.
 |  |  |  |  |  |  |
| 1. The flight recorder shall automatically start to record prior to the helicopter being capable of moving under its own power and shall stop automatically after the helicopter is no longer capable of moving under its own power.
 |  |  |  |  |  |  |
| 1. If the flight recorder records images or audio of the flight crew compartment, then a function shall be provided which can be operated by the commander and which modifies image and audio recordings made before the operation of that function, so that those recordings cannot be retrieved using normal replay or copying techniques.
 |  |  |  |  |  |  |

## CAT.IDE.H.195 Data link recording

|  |  |
| --- | --- |
| **Declaration of Compliance** | **Means of Compliance** |
| 1. Helicopters first issued with an individual CofA on or after 8 April 2014 that have the capability to operate data link communications and are required to be equipped with a CVR, shall record on a recorder, where applicable:
 | Requirement Satisfied | Requirement satisfied through type design as specified in Type Certificate Data Sheet (TCDS) | Requirement satisfied through Supplemental Type Certificate (STC) Process | Requirement satisfied through embodiment of manufacturer service publications (Service Bulletins, Service Changes, etc.) | Other  |
|  | (Note 1-4) | (Note 1) | (Note 2) | (Note 3) | (Note 4) |
|  | **Yes** | **N/A** |  |  |  |  |
| 1. data link communication messages related to ATS communications to and from the helicopter, including messages applying to the following applications:
 |  |
| 1. data link initiation;
 |[ ] [ ] [ ]        |       |       |
| 1. controller-pilot communication;
 |[ ] [ ] [ ]        |       |       |
| 1. addressed surveillance;
 |[ ] [ ] [ ]        |       |       |
| 1. flight information;
 |[ ] [ ] [ ]        |       |       |
| 1. as far as is practicable, given the architecture of the system, aircraft broadcast surveillance;
 |[ ] [ ] [ ]        |       |       |
| 1. as far as is practicable, given the architecture of the system, aircraft operational control data;
 |[ ] [ ] [ ]        |       |       |
| 1. as far as is practicable, given the architecture of the system, graphics;
 |[ ] [ ] [ ]        |       |       |
| 1. information that enables correlation to any associated records related to data link communications and stored separately from the helicopter; and
 |[ ] [ ] [ ]        |       |       |
| 1. information on the time and priority of data link communications messages, taking into account the system's architecture.
 |[ ] [ ] [ ]        |       |       |
| 1. The recorder shall use a digital method of recording and storing data and information and a method of readily retrieving that data shall be available. The recording method shall allow the data to match the data recorded on the ground.
 |[ ] [ ] [ ]        |       |       |
| 1. The recorder shall be capable of retaining data recorded for at least the same duration as set out for CVRs in CAT.IDE.H.185.
 |[ ] [ ] [ ]        |       |       |
| 1. If the recorder is not deployable, it shall have a device to assist in locating it under water. By 1 January 2020 at the latest, this device shall have a minimum underwater transmission time of 90 days. If the recorder is deployable, it shall have an automatic emergency locator transmitter.
 |[ ] [ ] [ ]        |       |       |
| 1. The requirements applicable to the start and stop logic of the recorder are the same as the requirements applicable to the start and stop logic of the CVR contained in CAT.IDE.H.185(d) and (e).
 |[ ] [ ] [ ]        |       |       |

## CAT.IDE.H.200 Flight data and cockpit voice combination recorder

|  |  |
| --- | --- |
| **Declaration of Compliance** | **Means of Compliance** |
|  | Requirement Satisfied | Requirement satisfied through type design as specified in Type Certificate Data Sheet (TCDS) | Requirement satisfied through Supplemental Type Certificate (STC) Process | Requirement satisfied through embodiment of manufacturer service publications (Service Bulletins, Service Changes, etc.) | Other  |
|  | (Note 1-4) | (Note 1) | (Note 2) | (Note 3) | (Note 4) |
|  | **Yes** | **N/A** |  |  |  |  |
| Compliance with CVR and FDR requirements may be achieved by the carriage of one combination recorder. |[ ] [ ] [ ]        |       |       |

## CAT.IDE.H.205 Seats, seat safety belts, restraint systems and child restraint devices

|  |  |
| --- | --- |
| **Declaration of Compliance** | **Means of Compliance** |
| 1. Helicopters shall be equipped with:
 | Requirement Satisfied | Requirement satisfied through type design as specified in Type Certificate Data Sheet (TCDS) | Requirement satisfied through Supplemental Type Certificate (STC) Process | Requirement satisfied through embodiment of manufacturer service publications (Service Bulletins, Service Changes, etc.) | Other  |
|  | (Note 1-4) | (Note 1) | (Note 2) | (Note 3) | (Note 4) |
|  | **Yes** | **N/A** |  |  |  |  |
| 1. a seat or berth for each person on board who is aged 24 months or more;
 |[ ] [ ] [ ]        |       |       |
| 1. a seat belt on each passenger seat and restraining belts for each berth;
 |[ ] [ ] [ ]        |       |       |
| 1. for helicopters first issued with an individual CofA on or after 1 August 1999, a safety belt with upper torso restraint system for use on each passenger seat for each passenger aged 24 months or more;
 |[ ] [ ] [ ]        |       |       |
| 1. a child restraint device (CRD) for each person on board younger than 24 months;
 |[ ] [ ] [ ]        |       |       |
| 1. a seat belt with upper torso restraint system incorporating a device that will automatically restrain the occupant's torso in the event of rapid deceleration on each flight crew seat;
 |[ ] [ ] [ ]        |       |       |
| 1. a seat belt with upper torso restraint system on each seat for the minimum required cabin crew.
 |[ ] [ ] [ ]        |       |       |
| 1. A seat belt with upper torso restraint system shall:
 |  |
| 1. have a single point release; and
 |[ ] [ ] [ ]        |       |       |
| 1. on flight crew seats and on the seats for the minimum required cabin crew include two shoulder straps and a seat belt that may be used independently.
 |[ ] [ ] [ ]        |       |       |

## CAT.IDE.H.210 Fasten seat belt and no smoking signs

|  |  |
| --- | --- |
| **Declaration of Compliance** | **Means of Compliance** |
|  | Requirement Satisfied | Requirement satisfied through type design as specified in Type Certificate Data Sheet (TCDS) | Requirement satisfied through Supplemental Type Certificate (STC) Process | Requirement satisfied through embodiment of manufacturer service publications (Service Bulletins, Service Changes, etc.) | Other  |
|  | (Note 1-4) | (Note 1) | (Note 2) | (Note 3) | (Note 4) |
|  | **Yes** | **N/A** |  |  |  |  |
| Helicopters in which not all passenger seats are visible from the flight crew seat(s) shall be equipped with a means of indicating to all passengers and cabin crew when seat belts shall be fastened and when smoking is not allowed. |[ ] [ ] [ ]        |       |       |

## CAT.IDE.H.220 First-aid kits

|  |  |
| --- | --- |
| **Declaration of Compliance** | **Means of Compliance** |
|  | Requirement Satisfied | Requirement satisfied through type design as specified in Type Certificate Data Sheet (TCDS) | Requirement satisfied through Supplemental Type Certificate (STC) Process | Requirement satisfied through embodiment of manufacturer service publications (Service Bulletins, Service Changes, etc.) | Other  |
|  | (Note 1-4) | (Note 1) | (Note 2) | (Note 3) | (Note 4) |
|  | **Yes** | **N/A** |  |  |  |  |
| 1. Helicopters shall be equipped with at least one first-aid kit.
 |[ ] [ ] [ ]        |       |       |
| 1. First-aid kits shall be:
 |  |
| 1. readily accessible for use;
 |[ ] [ ] [ ]        |       |       |
| 1. kept up to date.
 |[ ] [ ] [ ]        |       |       |

## CAT.IDE.H.240 Supplemental oxygen — non-pressurised helicopters

|  |  |
| --- | --- |
| **Declaration of Compliance** | **Means of Compliance** |
|  | Requirement Satisfied | Requirement satisfied through type design as specified in Type Certificate Data Sheet (TCDS) | Requirement satisfied through Supplemental Type Certificate (STC) Process | Requirement satisfied through embodiment of manufacturer service publications (Service Bulletins, Service Changes, etc.) | Other  |
|  | (Note 1-4) | (Note 1) | (Note 2) | (Note 3) | (Note 4) |
|  | **Yes** | **N/A** |  |  |  |  |
| Non-pressurised helicopters operated at pressure altitudes above 10’000 ft shall be equipped with supplemental oxygen equipment capable of storing and dispensing the oxygen supplies in accordance with the following tables. |[ ] [ ] [ ]        |       |       |

|  |  |  |
| --- | --- | --- |
| **Table 1 Oxygen minimum requirements for complex non-press. helicopters** |  | **Table 2 Oxygen minimum requirements for other-than-complex non-press. helicopters** |
|  | Supply for | Duration and cabin pressure altitude |  | Supply for | Duration and cabin pressure altitude |
| 1 | Occupants of flight crew compartment seats on flight crew compartment duty and crew members assisting flight crew in their duties | The entire flying time at pressure altitudes above 10’000 ft. | 1 | Occupants of flight crew compartment seats on flight crew compartment duty, crew members assisting flight crew in their duties, and required cabin crew members | The entire flying time at pressure altitudes above 13’000 ft and for any period exceeding 30 minutes at pressure altitudes above 10’000 ft but not exceeding 13’000 ft. |
| 2 | Required cabin crew members | The entire flying time at pressure altitudes above 13’000 ft and for any period exceeding 30 minutes at pressure altitudes above 10’000 ft but not exceeding 13’000 ft. | 2 | Additional crew members and 100 % of passengers \* | The entire flying time at pressure altitudes above 13’000 ft. |
| 3 | Additional crew members and 100 % of passengers \* | The entire flying time at pressure altitudes above 13’000 ft. | 3 | 10 % of passengers \* | The entire flying time after 30 minutes at pressure altitudes above 10’000 ft but not exceeding 13’000 ft. |
| 4 | 10 % of passengers \* | The entire flying time after 30 minutes at pressure altitudes above 10’000 ft but not exceeding 13’000 ft. | \* | Passenger numbers in Table 2 refer to passengers actually carried on board including persons younger than 24 months. |
| \* | Passenger numbers in Table 1 refer to passengers actually carried on board including persons younger than 24 months. |  |

## CAT.IDE.H.250 Hand fire extinguishers

|  |  |
| --- | --- |
| **Declaration of Compliance** | **Means of Compliance** |
|  | Requirement Satisfied | Requirement satisfied through type design as specified in Type Certificate Data Sheet (TCDS) | Requirement satisfied through Supplemental Type Certificate (STC) Process | Requirement satisfied through embodiment of manufacturer service publications (Service Bulletins, Service Changes, etc.) | Other  |
|  | (Note 1-4) | (Note 1) | (Note 2) | (Note 3) | (Note 4) |
|  | **Yes** | **N/A** |  |  |  |  |
| 1. Helicopters shall be equipped with at least one hand fire extinguisher in the flight crew compartment.
 |[ ] [ ] [ ]        |       |       |
| 1. At least one hand fire extinguisher shall be located in, or readily accessible for use in, each galley not located on the main passenger compartment.
 |[ ] [ ] [ ]        |       |       |
| 1. At least one hand fire extinguisher shall be available for use in each cargo compartment that is accessible to crew members in flight.
 |[ ] [ ] [ ]        |       |       |
| 1. The type and quantity of extinguishing agent for the required fire extinguishers shall be suitable for the type of fire likely to occur in the compartment where the extinguisher is intended to be used and to minimise the hazard of toxic gas concentration in compartments occupied by persons.
 |[ ] [ ] [ ]        |       |       |
| 1. The helicopter shall be equipped with at least a number of hand fire extinguishers in accordance with Table 1, conveniently located to provide adequate availability for use in each passenger compartment.
 |[ ] [ ] [ ]        |       |       |

|  |
| --- |
| **Table 1 Number of hand fire extinguishers** |
| **MOPSC** | **Number of extinguishers** |
| 7-30 | 1 |
| 31-60 | 2 |
| 61-200 | 3 |

## CAT.IDE.H.260 Marking of break-in points

|  |  |
| --- | --- |
| **Declaration of Compliance** | **Means of Compliance** |
|  | Requirement Satisfied | Requirement satisfied through type design as specified in Type Certificate Data Sheet (TCDS) | Requirement satisfied through Supplemental Type Certificate (STC) Process | Requirement satisfied through embodiment of manufacturer service publications (Service Bulletins, Service Changes, etc.) | Other  |
|  | (Note 1-4) | (Note 1) | (Note 2) | (Note 3) | (Note 4) |
|  | **Yes** | **N/A** |  |  |  |  |
| If areas of the helicopter's fuselage suitable for break-in by rescue crews in an emergency are marked, such areas shall be marked as shown in Figure 1. |[ ] [ ] [ ]        |       |       |

**Figure 1 Marking of break-in points**



## CAT.IDE.H.270 Megaphones

|  |  |
| --- | --- |
| **Declaration of Compliance** | **Means of Compliance** |
|  | Requirement Satisfied | Requirement satisfied through type design as specified in Type Certificate Data Sheet (TCDS) | Requirement satisfied through Supplemental Type Certificate (STC) Process | Requirement satisfied through embodiment of manufacturer service publications (Service Bulletins, Service Changes, etc.) | Other  |
|  | (Note 1-4) | (Note 1) | (Note 2) | (Note 3) | (Note 4) |
|  | **Yes** | **N/A** |  |  |  |  |
| Helicopters with an MOPSC of more than 19 shall be equipped with one portable battery-powered megaphone readily accessible for use by crew members during an emergency evacuation. |[ ] [ ] [ ]        |       |       |

## CAT.IDE.H.275 Emergency lighting and marking

|  |  |
| --- | --- |
| **Declaration of Compliance** | **Means of Compliance** |
| 1. Helicopters with an MOPSC of more than 19 shall be equipped with:
 | Requirement Satisfied | Requirement satisfied through type design as specified in Type Certificate Data Sheet (TCDS) | Requirement satisfied through Supplemental Type Certificate (STC) Process | Requirement satisfied through embodiment of manufacturer service publications (Service Bulletins, Service Changes, etc.) | Other  |
|  | (Note 1-4) | (Note 1) | (Note 2) | (Note 3) | (Note 4) |
|  | **Yes** | **N/A** |  |  |  |  |
| 1. an emergency lighting system having an independent power supply to provide a source of general cabin illumination to facilitate the evacuation of the helicopter; and
 |[ ] [ ] [ ]        |       |       |
| 1. emergency exit marking and locating signs visible in daylight or in the dark.
 |[ ] [ ] [ ]        |       |       |
| 1. Helicopters shall be equipped with emergency exit markings visible in daylight or in the dark when operated:
 |  |
| 1. in performance class 1 or 2 on a flight over water at a distance from land corresponding to more than 10 minutes flying time at normal cruising speed;
 |[ ] [ ] [ ]        |       |       |
| 1. in performance class 3 on a flight over water at a distance corresponding to more than three minutes flying time at normal cruising speed.
 |[ ] [ ] [ ]        |       |       |

## CAT.IDE.H.280 Emergency locator transmitter (ELT)

|  |  |
| --- | --- |
| **Declaration of Compliance** | **Means of Compliance** |
|  | Requirement Satisfied | Requirement satisfied through type design as specified in Type Certificate Data Sheet (TCDS) | Requirement satisfied through Supplemental Type Certificate (STC) Process | Requirement satisfied through embodiment of manufacturer service publications (Service Bulletins, Service Changes, etc.) | Other  |
|  | (Note 1-4) | (Note 1) | (Note 2) | (Note 3) | (Note 4) |
|  | **Yes** | **N/A** |  |  |  |  |
| 1. Helicopters shall be equipped with at least one automatic ELT.
 |[ ] [ ] [ ]        |       |       |
| 1. An ELT of any type shall be capable of transmitting simultaneously on 121.5 MHz and 406 MHz.
 |[ ] [ ] [ ]        |       |       |

## CAT.IDE.H.290 Life-jackets

|  |  |
| --- | --- |
| **Declaration of Compliance** | **Means of Compliance** |
| 1. Helicopters shall be equipped with a life-jacket for each person on board or equivalent floatation device for each person on board younger than 24 months, stowed in a position that is readily accessible from the seat or berth of the person for whose use it is provided, when operated in:
 | Requirement Satisfied | Requirement satisfied through type design as specified in Type Certificate Data Sheet (TCDS) | Requirement satisfied through Supplemental Type Certificate (STC) Process | Requirement satisfied through embodiment of manufacturer service publications (Service Bulletins, Service Changes, etc.) | Other  |
|  | (Note 1-4) | (Note 1) | (Note 2) | (Note 3) | (Note 4) |
|  | **Yes** | **N/A** |  |  |  |  |
| 1. performance class 1 or 2 on a flight over water at a distance from land corresponding to more than 10 minutes flying time at normal cruising speed;
 |[ ] [ ] [ ]        |       |       |
| 1. performance class 3 on a flight over water beyond autorotational distance from land;
 |[ ] [ ] [ ]        |       |       |
| 1. performance class 2 or 3 when taking off or landing at an aerodrome or operating site where the take-off or approach path is over water.
 |[ ] [ ] [ ]        |       |       |
| 1. Each life-jacket or equivalent individual flotation device shall be equipped with a means of electric illumination for the purpose of facilitating the location of persons.
 |[ ] [ ] [ ]        |       |       |

## CAT.IDE.H.295 Crew survival suits

|  |  |
| --- | --- |
| **Declaration of Compliance** | **Means of Compliance** |
|  | Requirement Satisfied | Requirement satisfied through type design as specified in Type Certificate Data Sheet (TCDS) | Requirement satisfied through Supplemental Type Certificate (STC) Process | Requirement satisfied through embodiment of manufacturer service publications (Service Bulletins, Service Changes, etc.) | Other  |
|  | (Note 1-4) | (Note 1) | (Note 2) | (Note 3) | (Note 4) |
|  | **Yes** | **N/A** |  |  |  |  |
| Each crew member shall wear a survival suit when operating in performance class 3 on a flight over water beyond autorotational distance or safe forced landing distance from land, when the weather report or forecasts available to the commander indicate that the sea temperature will be less than plus 10 °C during the flight. |[ ] [ ] [ ]        |       |       |

## CAT.IDE.H.300 Life-rafts, survival ELTs and survival equipment on extended overwater flights

|  |  |
| --- | --- |
| **Declaration of Compliance** | **Means of Compliance** |
| Helicopters operated: | Requirement Satisfied | Requirement satisfied through type design as specified in Type Certificate Data Sheet (TCDS) | Requirement satisfied through Supplemental Type Certificate (STC) Process | Requirement satisfied through embodiment of manufacturer service publications (Service Bulletins, Service Changes, etc.) | Other  |
|  | (Note 1-4) | (Note 1) | (Note 2) | (Note 3) | (Note 4) |
|  | **Yes** | **N/A** |  |  |  |  |
| 1. in performance class 1 or 2 on a flight over water at a distance from land corresponding to more than 10 minutes flying time at normal cruising speed;
 |[ ] [ ] [ ]        |       |       |
| 1. in performance class 3 on a flight over water at a distance corresponding to more than three minutes flying time at normal cruising speed, shall be equipped with:
 |  |
| 1. in the case of a helicopter carrying less than 12 persons, at least one life-raft with a rated capacity of not less than the maximum number of persons on board, stowed so as to facilitate its ready use in an emergency;
 |[ ] [ ] [ ]        |       |       |
| 1. in the case of a helicopter carrying more than 11 persons, at least two life-rafts, stowed so as to facilitate their ready use in an emergency, sufficient together to accommodate all persons capable of being carried on board and, if one is lost, the remaining life-raft(s) having, the overload capacity sufficient to accommodate all persons on the helicopter;
 |[ ] [ ] [ ]        |       |       |
| 1. at least one survival ELT (ELT(S)) for each required life-raft; and
 |[ ] [ ] [ ]        |       |       |
| 1. life-saving equipment, including means of sustaining life, as appropriate to the flight to be undertaken.
 |[ ] [ ] [ ]        |       |       |

## CAT.IDE.H.305 Survival equipment

|  |  |
| --- | --- |
| **Declaration of Compliance** | **Means of Compliance** |
| Helicopters operated over areas in which search and rescue would be especially difficult shall be equipped with: | Requirement Satisfied | Requirement satisfied through type design as specified in Type Certificate Data Sheet (TCDS) | Requirement satisfied through Supplemental Type Certificate (STC) Process | Requirement satisfied through embodiment of manufacturer service publications (Service Bulletins, Service Changes, etc.) | Other  |
|  | (Note 1-4) | (Note 1) | (Note 2) | (Note 3) | (Note 4) |
|  | **Yes** | **N/A** |  |  |  |  |
| 1. signalling equipment to make distress signals;
 |[ ] [ ] [ ]        |       |       |
| 1. at least one ELT(S); and
 |[ ] [ ] [ ]        |       |       |
| 1. additional survival equipment for the route to be flown taking account of the number of persons on board.
 |[ ] [ ] [ ]        |       |       |

## CAT.IDE.H.315 Helicopters certified for operating on water — miscellaneous equipment

|  |  |
| --- | --- |
| **Declaration of Compliance** | **Means of Compliance** |
| Helicopters certified for operating on water shall be equipped with: | Requirement Satisfied | Requirement satisfied through type design as specified in Type Certificate Data Sheet (TCDS) | Requirement satisfied through Supplemental Type Certificate (STC) Process | Requirement satisfied through embodiment of manufacturer service publications (Service Bulletins, Service Changes, etc.) | Other  |
|  | (Note 1-4) | (Note 1) | (Note 2) | (Note 3) | (Note 4) |
|  | **Yes** | **N/A** |  |  |  |  |
| 1. a sea anchor and other equipment necessary to facilitate mooring, anchoring or manoeuvring the helicopter on water, appropriate to its size, weight and handling characteristics; and
 |[ ] [ ] [ ]        |       |       |
| 1. equipment for making the sound signals prescribed in the International Regulations for Preventing Collisions at Sea, where applicable.
 |[ ] [ ] [ ]        |       |       |

## CAT.IDE.H.320 All helicopters on flights over water — ditching

|  |  |
| --- | --- |
| **Declaration of Compliance** | **Means of Compliance** |
|  | Requirement Satisfied | Requirement satisfied through type design as specified in Type Certificate Data Sheet (TCDS) | Requirement satisfied through Supplemental Type Certificate (STC) Process | Requirement satisfied through embodiment of manufacturer service publications (Service Bulletins, Service Changes, etc.) | Other  |
|  | (Note 1-4) | (Note 1) | (Note 2) | (Note 3) | (Note 4) |
|  | **Yes** | **N/A** |  |  |  |  |
| 1. Helicopters shall be designed for landing on water or certified for ditching in accordance with the relevant certification specification when operated in performance class 1 or 2 on a flight over water in a hostile environment at a distance from land corresponding to more than 10 minutes flying time at normal cruise speed.
 |[ ] [ ] [ ]        |       |       |
| 1. Helicopters shall be designed for landing on water or certified for ditching in accordance with the relevant certification specification or fitted with emergency flotation equipment when operated in:
 |  |
| 1. performance class 1 or 2 on a flight over water in a non-hostile environment at a distance from land corresponding to more than 10 minutes flying time at normal cruise speed;
 |[ ] [ ] [ ]        |       |       |
| 1. performance class 2, when taking off or landing over water, except in the case of helicopter emergency medical services (HEMS) operations, where for the purpose of minimising exposure, the landing or take-off at a HEMS operating site located in a congested environment is conducted over water;
 |[ ] [ ] [ ]        |       |       |
| 1. performance class 3 on a flight over water beyond safe forced landing distance from land.
 |[ ] [ ] [ ]        |       |       |

## CAT.IDE.H.325 Headset

|  |  |
| --- | --- |
| **Declaration of Compliance** | **Means of Compliance** |
|  | Requirement Satisfied | Requirement satisfied through type design as specified in Type Certificate Data Sheet (TCDS) | Requirement satisfied through Supplemental Type Certificate (STC) Process | Requirement satisfied through embodiment of manufacturer service publications (Service Bulletins, Service Changes, etc.) | Other  |
|  | (Note 1-4) | (Note 1) | (Note 2) | (Note 3) | (Note 4) |
|  | **Yes** | **N/A** |  |  |  |  |
| Whenever a radio communication and/or radio navigation system is required, helicopters shall be equipped with a headset with boom microphone or equivalent and a transmit button on the flight controls for each required pilot and/or crew member at his/her assigned station. |[ ] [ ] [ ]        |       |       |

## CAT.IDE.H.330 Radio communication equipment

|  |  |
| --- | --- |
| **Declaration of Compliance** | **Means of Compliance** |
|  | Requirement Satisfied | Requirement satisfied through type design as specified in Type Certificate Data Sheet (TCDS) | Requirement satisfied through Supplemental Type Certificate (STC) Process | Requirement satisfied through embodiment of manufacturer service publications (Service Bulletins, Service Changes, etc.) | Other  |
|  | (Note 1-4) | (Note 1) | (Note 2) | (Note 3) | (Note 4) |
|  | **Yes** | **N/A** |  |  |  |  |
| 1. Helicopters shall be equipped with the radio communication equipment required by the applicable airspace requirements.
 |[ ] [ ] [ ]        |       |       |
| 1. The radio communication equipment shall provide for communication on the aeronautical emergency frequency 121.5 MHz.
 |[ ] [ ] [ ]        |       |       |

## CAT.IDE.H.335 Audio selector panel

|  |  |
| --- | --- |
| **Declaration of Compliance** | **Means of Compliance** |
|  | Requirement Satisfied | Requirement satisfied through type design as specified in Type Certificate Data Sheet (TCDS) | Requirement satisfied through Supplemental Type Certificate (STC) Process | Requirement satisfied through embodiment of manufacturer service publications (Service Bulletins, Service Changes, etc.) | Other  |
|  | (Note 1-4) | (Note 1) | (Note 2) | (Note 3) | (Note 4) |
|  | **Yes** | **N/A** |  |  |  |  |
| Helicopters operated under IFR shall be equipped with an audio selector panel operable from each required flight crew member station. |[ ] [ ] [ ]        |       |       |

## CAT.IDE.H.340 Radio equipment for operations under VFR over routes navigated by reference to visual landmarks

|  |  |
| --- | --- |
| **Declaration of Compliance** | **Means of Compliance** |
| Helicopters operated under VFR over routes that can be navigated by reference to visual landmarks shall be equipped with radio communication equipment necessary under normal radio propagation conditions to fulfil the following: | Requirement Satisfied | Requirement satisfied through type design as specified in Type Certificate Data Sheet (TCDS) | Requirement satisfied through Supplemental Type Certificate (STC) Process | Requirement satisfied through embodiment of manufacturer service publications (Service Bulletins, Service Changes, etc.) | Other  |
|  | (Note 1-4) | (Note 1) | (Note 2) | (Note 3) | (Note 4) |
|  | **Yes** | **N/A** |  |  |  |  |
| 1. communicate with appropriate ground stations;
 |[ ] [ ] [ ]        |       |       |
| 1. communicate with appropriate ATC stations from any point in controlled airspace within which flights are intended; and
 |[ ] [ ] [ ]        |       |       |
| 1. receive meteorological information.
 |[ ] [ ] [ ]        |       |       |

## CAT.IDE.H.345 Communication and navigation equipment for operations under IFR or under VFR over routes not navigated by reference to visual landmarks

|  |  |
| --- | --- |
| **Declaration of Compliance** | **Means of Compliance** |
|  | Requirement Satisfied | Requirement satisfied through type design as specified in Type Certificate Data Sheet (TCDS) | Requirement satisfied through Supplemental Type Certificate (STC) Process | Requirement satisfied through embodiment of manufacturer service publications (Service Bulletins, Service Changes, etc.) | Other  |
|  | (Note 1-4) | (Note 1) | (Note 2) | (Note 3) | (Note 4) |
|  | **Yes** | **N/A** |  |  |  |  |
| 1. Helicopters operated under IFR or under VFR over routes that cannot be navigated by reference to visual landmarks shall be equipped with radio communication, navigation and surveillance equipment in accordance with the applicable airspace requirements.
 |[ ] [ ] [ ]        |       |       |
| 1. Radio communication equipment shall include at least two independent radio communication systems necessary under normal operating conditions to communicate with an appropriate ground station from any point on the route, including diversions.
 |[ ] [ ] [ ]        |       |       |
| 1. Helicopters shall have sufficient navigation equipment to ensure that, in the event of the failure of one item of equipment at any stage of the flight, the remaining equipment shall allow safe navigation in accordance with the flight plan
 |[ ] [ ] [ ]        |       |       |
| 1. Helicopters operated on flights in which it is intended to land in IMC shall be equipped with suitable equipment capable of providing guidance to a point from which a visual landing can be performed for each aerodrome at which it is intended to land in IMC and for any designated alternate aerodromes.
 |[ ] [ ] [ ]        |       |       |
| 1. For PBN operations the aircraft shall meet the airworthiness certification requirements for the appropriate navigation specification.
 |[ ] [ ] [ ]        |       |       |

## CAT.IDE.H.350 Transponder

|  |  |
| --- | --- |
| **Declaration of Compliance** | **Means of Compliance** |
|  | Requirement Satisfied | Requirement satisfied through type design as specified in Type Certificate Data Sheet (TCDS) | Requirement satisfied through Supplemental Type Certificate (STC) Process | Requirement satisfied through embodiment of manufacturer service publications (Service Bulletins, Service Changes, etc.) | Other  |
|  | (Note 1-4) | (Note 1) | (Note 2) | (Note 3) | (Note 4) |
|  | **Yes** | **N/A** |  |  |  |  |
| Helicopters shall be equipped with a pressure altitude reporting secondary surveillance radar (SSR) transponder and any other SSR transponder capability required for the route being flown. |[ ] [ ] [ ]        |       |       |

## CAT.IDE.H.355 Management of aeronautical databases

|  |  |
| --- | --- |
| **Declaration of Compliance** | **Means of Compliance** |
|  | Requirement Satisfied | Requirement satisfied through type design as specified in Type Certificate Data Sheet (TCDS) | Requirement satisfied through Supplemental Type Certificate (STC) Process | Requirement satisfied through embodiment of manufacturer service publications (Service Bulletins, Service Changes, etc.) | Other  |
|  | (Note 1-4) | (Note 1) | (Note 2) | (Note 3) | (Note 4) |
|  | **Yes** | **N/A** |  |  |  |  |
| 1. Aeronautical databases used on certified aircraft system applications shall meet data quality requirements that are adequate for the intended use of the data.
 |[ ] [ ] [ ]        |       |       |
| 1. The operator shall ensure the timely distribution and insertion of current and unaltered aeronautical databases to all aircraft that require them.
 |[ ] [ ] [ ]        |       |       |
| 1. Notwithstanding any other occurrence reporting requirements as defined in Regulation (EU) No 376/2014, the operator shall report to the database provider instances of erroneous, inconsistent or missing data that might be reasonably expected to constitute a hazard to flight.

In such cases, the operator shall inform flight crew and other personnel concerned, and shall ensure that the affected data is not used. |[ ] [ ] [ ]        |       |       |

# Applicant’s Statement

I herewith confirm correctness of the EASA (EC 2018/1139) Air Operations Regulation Annex IV, Part-CAT.IDE (incl. Annex III, ORO.SEC) Compliance List and accept that any false claims identified by FOCA during their subsequent inspection may lead to legal action.

|  |  |  |  |
| --- | --- | --- | --- |
| Postholder Cont. Airworth. PCA |      Name |      Signature |      Date |

|  |  |  |  |
| --- | --- | --- | --- |
| Nominated Person Flight Ops.\* |      Name |      Signature |      Date |

\*Chief Flight Ops

|  |  |  |  |
| --- | --- | --- | --- |
|  | **AWI**Evaluation completed | This EASA ORO.SEC/CAT.IDE compliance statement,taking regard to AOC operation, only attests compliance withthe pertinent technical aspects. The final AOC privileges shall be officially registered not before the corresponding**STSS/Regis** evaluation tasks have been signed off. |  |
| Date:Sign.: |  | **FOCA** |